{"text_format":"3","workbook":"xlsx","n_sheets":5,"sheets":["Allgemeines","Equipment","Baudokumentation","Flugeinstellungen","Flugbuch"],"not_rendered":{"macros":1,"defined_names":2,"comments":1},"read":"whole","date_system":"1900"}

{"sheet":"Allgemeines","index":0,"n_rows":45,"n_cols":13,"rows_kept":45,"merged":[[1,1,1,2],[1,5,1,9],[1,11,1,12],[2,1,15,1],[2,4,15,12],[16,1,34,1],[16,2,22,2],[16,8,34,8],[17,9,29,9],[23,2,25,2],[27,2,31,2],[30,9,33,9],[32,2,34,2],[35,1,41,1],[41,10,41,12]]}
[]
[null,"Modellname",null,"#",{"$nulls":6},"Stand:","2018-01-15T16:16:29"]
[null,"Basics","Pilot","#","3-Seiten-Ansicht / Bild"]
[null,null,"Kategorie","(E-)Segelflugmodell"]
[null,null,"Antrieb","ja"]
[null,null,"Leitwerksart","V-Leitwerk"]
[null,null,"im Betrieb seit","#"]
[null,null,"im Betrieb bis","#"]
[null,null,"Hersteller","#"]
[null,null,"evtl. Vorbesitzer","#"]
[null,null,"Kaufpreis","#"]
[null,null,"evtl. Nachbesitzer","#"]
[null,null,"Verkaufspreis","#"]
[null,null,"Profil FL","#"]
[null,null,"Profil LW","#"]
[]
[null,"Geometrie","Spannweite","FL projiziert",null,"#","mm",null,"Gewichte","Startgewicht","gesamt","#","g"]
[{"$nulls":3},"FL links",null,"#","mm",null,null,"Einzelgewichte","FL links","#","g"]
[{"$nulls":3},"FL mitte",null,"#","mm",{"$nulls":3},"FL mitte","#","g"]
[{"$nulls":3},"FL rechts",null,"#","mm",{"$nulls":3},"FL rechts","#","g"]
[{"$nulls":3},"HR (V-LW projiziert)",null,"#","mm",{"$nulls":3},"LW links","#","g"]
[{"$nulls":3},"SR (V-LW projiziert)",null,"#","mm",{"$nulls":3},"LW mitte","#","g"]
[{"$nulls":3},"V-LW-Hälfte absolut",null,"#","mm",{"$nulls":3},"LW rechts","#","g"]
[null,null,"Flächeninhalt","FL projiziert",null,"#","dm²",{"$nulls":3},"Rumpf","#","g"]
[{"$nulls":3},"HR (V-LW projiziert)",null,"#","dm²",{"$nulls":3},"Nase","#","g"]
[{"$nulls":3},"SR (V-LW projiziert)",null,"#","dm²",{"$nulls":3},"Akku 1","#","g"]
[null,null,"Rumpflänge","gesamt",null,"#","mm",{"$nulls":3},"Akku 2","#","g"]
[null,null,"Einzelmaße","Nase bis NL FL",null,"#","mm",{"$nulls":3},"Akku 3","#","g"]
[{"$nulls":3},"Tiefe FL",null,"#","mm",{"$nulls":3},"Empfängerakku","#","g"]
[{"$nulls":3},"EL FL bis NL LW",null,"#","mm",{"$nulls":3},"Verbinder","#","g"]
[{"$nulls":3},"Tiefe LW",null,"#","mm",null,null,"Ballast","gesamt","#","g"]
[{"$nulls":3},"EL LW bis Rumpfende",null,"#","mm",{"$nulls":3},"Rumpf","#","g"]
[null,null,"V-Form","FL innen",null,"#","°",{"$nulls":3},"FL gesamt","#","g"]
[{"$nulls":3},"FL außen (3-teiliger FL)",null,"#","°",{"$nulls":3},"Verbinder","#","g"]
[{"$nulls":3},"LW",null,"#","°",null,null,"Flächenbelastung",{"$f":"L17/F24","v":{"$error":"#VALUE!"}},"g/dm²"]
[null,"Abkürzungen","FL","Flügel",null,"SR","Seitenruder"]
[null,null,"LW","Leitwerk",null,"HR","Höhenruder"]
[null,null,"NL","Nasenleiste",null,"QR","Querruder"]
[null,null,"EL","Endleiste",null,"WK","Wölbklappen"]
[null,null,"FR","Flugrichtung",null,"SK","Störklappen"]
[{"$nulls":5},"M","Motor"]
[{"$nulls":5},"B","Bremse"]
[]
[{"$nulls":9},"by Martin Petrich 01/2018  ","martin@bastelkellair.de"]
[{"$nulls":8},"Freigegeben zur privaten, nicht-kommerziellen Benutzung!"]

{"sheet":"Equipment","index":1,"n_rows":29,"n_cols":9,"rows_kept":29,"merged":[[1,1,1,2],[2,1,10,1],[11,1,22,1],[23,1,27,1]]}
[]
[null,{"$f":"Allgemeines!D2","v":"#"},null,"Hersteller","Typ","Lieferant","Datum","Kosten","Bemerkungen"]
[null,"Antrieb","Motor"]
[null,null,"Getriebe"]
[null,null,"Regler"]
[null,null,"Spinner"]
[null,null,"Luftschraube"]
[null,null,"Akku 1"]
[null,null,"Akku 2"]
[null,null,"Akku 3"]
[null,null,"Akkuweiche"]
[null,"Servos","F-Schlepp"]
[null,null,"Fahrwerk"]
[null,null,"Klapptriebwerk"]
[null,null,"Höhenruder"]
[null,null,"Seitenruder"]
[null,null,"V-Leitwerk"]
[null,null,"Querruder links"]
[null,null,"Wölbklappe links"]
[null,null,"Störklappe links"]
[null,null,"Störklappe rechts"]
[null,null,"Wölbklappe rechts"]
[null,null,"Querruder rechts"]
[null,"Allgemein","Empfänger"]
[null,null,"Akku"]
[null,null,"BEC"]
[null,null,"Akkuweiche"]
[null,null,"Spannungsstabil."]
[{"$nulls":5},"Gesamtkosten",null,{"$f":"SUM(H3:H28)","v":{"v":0,"d":"0.00 €"}},"by Martin Petrich 01/2018"]

{"sheet":"Baudokumentation","index":2,"n_rows":57,"n_cols":7,"rows_kept":57,"merged":[[1,2,1,3],[2,1,13,1],[2,2,7,2],[8,2,9,2],[14,1,23,1],[14,2,16,2],[17,2,21,2],[24,1,33,1],[24,2,26,2],[27,2,31,2],[34,1,45,1],[34,2,39,2],[40,2,41,2],[46,1,55,1],[46,2,50,2]]}
[]
[null,null,{"$f":"Allgemeines!D2","v":"#"},null,"Beschreibung","Kosten","Bemerkungen"]
[null,"Flügel","Aufbau","Lack"]
[{"$nulls":3},"Außenlage(n)"]
[{"$nulls":3},"Stützstoff"]
[{"$nulls":3},"Innenlage(n)"]
[{"$nulls":3},"D-Box"]
[{"$nulls":3},"Ruder"]
[null,null,"Holm","Gurt"]
[{"$nulls":3},"Steg"]
[{"$nulls":3},"Servoeinbau"]
[{"$nulls":3},"Verbinder"]
[{"$nulls":3},"Akkueinbau"]
[{"$nulls":3},"Rohbaugewicht"]
[null,"Rumpf","Aufbau","Lack"]
[{"$nulls":3},"Lagen"]
[{"$nulls":3},"Nasenbereich"]
[null,null,"Einbau","Servoeinbau"]
[{"$nulls":3},"Gestängeverlegung"]
[{"$nulls":3},"Empfängereinbau"]
[{"$nulls":3},"Akkueinbau"]
[{"$nulls":3},"Antennenverlegung"]
[{"$nulls":3},"Trimmblei"]
[{"$nulls":3},"Flitschenhaken"]
[null,"Aufstecknase","Aufbau","Lack"]
[{"$nulls":3},"Lagen"]
[{"$nulls":3},"Nasenbereich"]
[null,null,"Einbau","Servoeinbau"]
[{"$nulls":3},"Gestängeverlegung"]
[{"$nulls":3},"Empfängereinbau"]
[{"$nulls":3},"Akkueinbau"]
[{"$nulls":3},"Antennenverlegung"]
[{"$nulls":3},"Trimmblei"]
[{"$nulls":3},"Flitschenhaken"]
[null,"Leitwerk","Aufbau","Lack"]
[{"$nulls":3},"Außenlage(n)"]
[{"$nulls":3},"Stützstoff"]
[{"$nulls":3},"Innenlage(n)"]
[{"$nulls":3},"D-Box"]
[{"$nulls":3},"Ruder"]
[null,null,"Holm","Gurt"]
[{"$nulls":3},"Steg"]
[{"$nulls":3},"Servoeinbau"]
[{"$nulls":3},"Verbinder"]
[{"$nulls":3},"Akkueinbau"]
[{"$nulls":3},"Rohbaugewicht"]
[null,"Sonstiges","Kleinteile","   Gestänge"]
[{"$nulls":3},"   Kabel"]
[{"$nulls":3},"   Stecker"]
[{"$nulls":3},"   Goldkontakte"]
[{"$nulls":3},"   Schrumpfschlauch"]
[{"$nulls":3},"Schutztaschen"]
[{"$nulls":3},"Transportbox"]
[]
[]
[]
[{"$nulls":4},"Gesamtkosten",{"$f":"SUM(F3:F56)","v":{"v":0,"d":"0.00 €"}},"by Martin Petrich 01/2018"]

{"sheet":"Flugeinstellungen","index":3,"n_rows":43,"n_cols":20,"rows_kept":43,"merged":[[1,1,1,9],[1,11,1,19],[2,1,2,2],[2,3,2,4],[2,5,2,6],[2,7,2,8],[3,3,3,4],[3,5,3,6],[3,7,3,8],[4,3,4,4],[4,5,4,6],[4,7,4,8],[5,3,5,4],[5,5,5,6],[5,7,5,8],[6,3,6,4],[6,5,6,6],[6,7,6,8],[7,3,7,4],[7,5,7,6],[7,7,7,8],[9,1,9,19],[10,1,11,2],[10,3,10,4],[10,5,10,6],[10,7,10,8],[10,9,10,10],[10,11,10,12],[10,13,10,14],[10,15,10,16],[10,17,10,18],[12,1,17,1],[18,1,23,1],[24,1,34,1],[36,1,36,19],[37,1,42,1]]}
[]
[null,"Allgemeines",{"$nulls":9},"Legende"]
[null,{"$f":"Allgemeines!D2","v":"#"},null,"Normal",null,"Thermik",null,"Speed",{"$nulls":3},"Anstellwinkel ",null,null,"+","NL in FR höher als EL"]
[null,null,"Schwerpunkt ab NL","#",null,"#",null,"#",null,"mm",{"$nulls":4},"-","NL in FR niedriger als EL"]
[null,null,"Anstellwinkel FL","#",null,"#",null,"#",null,"°",null,"Ausschlag",null,null,"+","HR ↑ | QR/WK ↓"]
[null,null,"Anstellwinkel LW","#",null,"#",null,"#",null,"°",{"$nulls":4},"-","HR ↓ | QR/WK ↑"]
[null,null,"EWD","#",null,"#",null,"#",null,"°"]
[null,null,"Ballast","#",null,"#",null,"#",null,"g"]
[]
[null,"Ruderausschläge und Einstellwerte"]
[null,{"$f":"Allgemeines!D2","v":"#"},null,"Normal",null,"Start",null,"Landung",null,"Speed",null,"Thermik 1",null,"Thermik 2",null,"Strecke 1",null,"Strecke 2"]
[{"$nulls":3},"+","-","+","-","+","-","+","-","+","-","+","-","+","-","+","-"]
[null,"Neutrallage","Höhenruder",{"$nulls":16},"mm"]
[null,null,"Seitenruder",{"$nulls":16},"mm"]
[null,null,"Querruder",{"$nulls":16},"mm"]
[null,null,"Wölbklappe",{"$nulls":16},"mm"]
[null,null,"Störklappe",{"$nulls":16},"mm"]
[null,null,"Motor",{"$nulls":16},"mm"]
[null,"Endlage","Höhenruder",{"$nulls":16},"mm"]
[null,null,"Seitenruder",{"$nulls":16},"mm"]
[null,null,"Querruder",{"$nulls":16},"mm"]
[null,null,"Wölbklappe",{"$nulls":16},"mm"]
[null,null,"Störklappe",{"$nulls":16},"mm"]
[null,null,"Motor",{"$nulls":16},"mm"]
[null,"Mischer","Combi Switch (QR↦SR)",{"$nulls":16},"%"]
[null,null,"Snap Flap (HR↦WK)",{"$nulls":16},"%"]
[null,null,"Snap Flap (HR↦QR)",{"$nulls":16},"%"]
[null,null,"WK-Mitnahme (QR↦WK)",{"$nulls":16},"%"]
[null,null,"Butterfly (B↦QR)",{"$nulls":16},"%"]
[null,null,"Butterfly (B↦WK)",{"$nulls":16},"%"]
[null,null,"Butterfly (B↦HR)",{"$nulls":16},"%"]
[null,null,"M ↦ HR",{"$nulls":16},"%"]
[null,null,"Differenzierung QR",{"$nulls":16},"%"]
[null,null,"Differenzierung WK",{"$nulls":16},"%"]
[null,null,"Differenzierungs-Reduktion",{"$nulls":16},"%"]
[]
[null,"Sonstiges "]
[null,null,"Butterfly","nur in Flugphase Normal aktiv"]
[null,null,"Motor","auf 3-Stufen Schalter mit 0-60-100%"]
[]
[]
[]
[{"$nulls":19},"by Martin Petrich 01/2018"]

{"sheet":"Flugbuch","index":4,"n_rows":2,"n_cols":9,"rows_kept":2}
["Datum","Ort","Wetter","Windst. [bft]","Windr.","Flugzeit [min]","Motorlauf-zeit [min]","Akku","Bemerkungen"]
[{"$nulls":8},"Erstflug"]